**TOWN OF LEBANON**

**INVITATION TO BID**

**Aspinall Rec. Fields Dugout Slabs**

The Town of Lebanon is soliciting bids from qualified contractors for the installation of 4 concrete pads for dugouts at Aspinall Recreational Fields 479 Exeter Rd., Lebanon, CT. Bids will be received at the Office of the First Selectman, Town of Lebanon, 579 Exeter Road, Lebanon, CT 06249 until 3:00 pm on February 28, 2020.Bids shall be submitted in sealed envelopes labeled “Dugout Slabs Bid” and the contractor’s name and address clearly written on it.All questions shall be directed to Jason Nowosad, Facilities Director in writing at Town Hall, 579 Exeter Road, Lebanon, CT 06249 or via email (jnowosad@lebanonct.gov) or phone 860.642.6028. The Board of Selectmen reserves the right to reject any and all bids. The Town of Lebanon is an Equal Opportunity Employer.

**General Description**

The project shall consist of site preparation, the providing of 4 (qty) 8' x 20' concrete slabs constructed per attached Slab Detail, and site restoration at Lebanon's Aspinall Recreational Fields, 479 Exeter Road, Lebanon, CT 06249.

**Scope of Work**

All bids shall include all costs associated with labor, materials, equipment, etc. to complete all work described herein with no exceptions.

1. Site Preparation

* 1. All sites shall have all top soil, old piers, and other obstructions removed from the work area.

1.1.1. Field 2, 1st Base line dugout will require an approximately 3' high retaining wall approximately 6' long on one side and 22' along the backside. An 8" poured rebar reinforced concrete wall on a 10" thick x 16" wide footing may be utilized, other methods are may be submitted.

1.1.2. Field 3, 3rd base line dugout will require 1-1/4" crushed stone, filter fabric and a 6" perforated pipe to be placed under it in the line of an existing drainage swale.

 1.2. 1-1/4" processed gravel shall be placed in lifts no greater than 10" and compacted as needed at each site.

2. Concrete

 2.1. Provide 8' x 20' concrete slabs per the attached slab detail. Please indicate in your proposal your method of doing so. (i.e. ready mix, mobile mix, precast, etc.)

3. Site Restoration

 3.1 Place screened topsoil around entire slab, sloped away from the slab.

 3.2 Repair all damage to lawn areas due to construction activity/traffic.

**Bid Requirements**

All bidders shall provide proof of liability insurance and worker's compensation insurance in the form of an insurance certificate. The winning bidder shall provide an Insurance certificate naming Town of Lebanon as additional insured.

Bids shall include all costs associated with the work herein described. Any modifications suggested may be submitted as an add alternate

Bidder shall complete all work associated with the contract within 30 days of bid award.